{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["台式机","便携式","打印机","空调机","复印机","传真机","扫描仪","复印纸","碎纸机"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"台式机","index":0,"n_rows":103,"n_cols":10,"rows_kept":103,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,13],[3,0,3,1],[3,2,3,3],[4,0,4,1],[4,2,4,3],[5,0,14,1],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,0,16,1],[15,2,15,3],[16,2,16,3],[17,0,19,1],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,0,21,1],[20,2,20,3],[21,2,21,3],[22,0,23,1],[22,2,22,3],[23,2,23,3],[24,0,26,1],[24,2,24,3],[25,2,25,3],[26,2,26,3],[27,0,28,1],[27,2,27,3],[28,2,28,3],[29,0,29,1],[29,2,29,3],[30,0,30,1],[30,2,30,3],[31,0,31,1],[31,2,31,3],[32,0,32,1],[32,2,32,3],[33,0,33,1],[33,2,33,3],[34,0,34,2],[35,0,35,2],[36,0,36,2],[37,0,38,2],[39,0,39,2],[40,0,41,2],[40,3,41,3],[40,4,41,4],[40,5,41,5],[40,6,41,6],[40,7,41,7],[40,8,41,8],[40,9,41,9],[42,0,42,2],[43,0,43,2],[44,0,44,2],[45,0,45,3],[45,4,45,9],[46,0,46,3],[48,0,48,9],[49,0,49,9],[50,0,50,1],[50,2,50,3],[51,0,52,1],[51,2,52,3],[51,4,52,4],[53,0,53,1],[53,2,53,3],[54,0,54,1],[54,2,54,3],[55,0,60,1],[55,2,60,3],[61,0,61,1],[61,2,61,3],[62,0,62,1],[62,2,62,3],[63,0,63,1],[63,2,63,3],[64,0,64,1],[64,2,64,3],[65,0,65,2],[66,0,66,2],[67,0,67,2],[68,0,68,2],[69,0,73,2],[69,3,71,3],[72,3,73,3],[72,4,73,4],[74,0,74,2],[75,0,75,2],[76,0,76,2],[77,0,77,2],[78,0,78,2],[79,0,79,2],[80,0,80,2],[82,0,82,5],[83,0,83,9],[84,0,84,1],[84,2,84,3],[85,0,88,1],[85,2,88,3],[89,0,91,1],[89,2,91,3],[92,0,93,1],[92,2,93,3],[94,0,94,1],[94,2,94,3],[95,0,95,1],[95,2,95,3],[96,0,96,1],[96,2,96,3],[97,0,102,1],[97,2,102,3]],"flags":["formulas_cached_only"]}
["附件：2013年中央预算单位批量集中采购品目配置参考"]
["2013年台式计算机配置参考"]
["一、基本配置"]
[null,null,"配置",null,"配置一","配置二","配置三","一体机一","一体机二","安全可信"]
["价格",{"$nulls":3},"6000元","5000元","4000元","4500元","3500元","4500元"]
["显示器",null,"材质",null,"TN-扭曲向列","TN-扭曲向列","TN-扭曲向列","TN-扭曲向列","TN-扭曲向列","TN-扭曲向列"]
[null,null,"显示技术",null,"LED","LED","LED","LED","LED","LED"]
[null,null,"尺寸",null,"21.5寸","19寸","19寸","20寸","20寸","19寸"]
[null,null,"宽屏",null,"宽屏","宽屏","宽屏","宽屏","宽屏","宽屏"]
[null,null,"分辨率",null,"1920×1080","1440×900","1440×900","1600*900","1600*900","1440×900"]
[null,null,"响应时间",null,"5ms","5ms","5ms","5ms","5ms","5ms"]
[null,null,"接口",null,"支持数字接口","支持数字接口","支持数字接口","支持数字接口","支持数字接口","支持数字接口"]
[null,null,"可视角度",null,"≥160°/160°","≥160°/160°","≥160°/160°","≥160°/160°","≥160°/160°","≥160°/160°"]
[null,null,"刷新率",null,"≥60Hz","≥60Hz","≥60Hz","≥60Hz","≥60Hz","≥60Hz"]
[null,null,"亮度",null,"250cd/m²","250cd/m²","250cd/m²","250cd/m²","250cd/m²","250cd/m²"]
["CPU",null,"核心数",null,"≥4核","≥2核","≥2核","≥2核\n","≥2核\n","≥2核"]
[null,null,"速度",null,"≥3.2GHz","≥3.2GHz","≥3.0GHz","主频≥2.6GHz","主频≥2.6GHz","主频≥2.6GHz"]
["硬盘",null,"硬盘容量",null,"1TB","1TB","500GB","≥500GB","≥500GB","≥320GB"]
[null,null,"接口类型",null,"SATAIII","SATAIII","SATAIII","SATAIII","SATAIII","SATAIII"]
[null,null,"转速",null,"7200转","7200转","7200转","7200转","7200转","7200转"]
["内存",null,"容量",null,"4GB","4GB","2GB","2GB","2GB","2GB"]
[null,null,"频率",null,"≥1333MHz","≥1333MHz","≥1333MHz","≥1333MHz","≥1333MHz","≥1333MHz"]
["显卡",null,"类型",null,"独立显卡（支持数字接口）","独立显卡（支持数字接口）","集成显卡","独立显卡（支持数字接口）","集成显卡","集成显卡"]
[null,null,"显存容量",null,"1GB","512MB","动态分布","1GB","动态分布","动态分布"]
["光驱",null,"类型",null,"≥DVD刻录","≥DVD刻录","≥DVD刻录","≥DVD只读","≥DVD只读","≥DVD只读"]
[null,null,"接口",null,"SATA","SATA","SATA","SATA","SATA","SATA"]
[null,null,"倍速",null,"16X","16X","16X","16X","16X","16X"]
["网卡",null,"有线网卡",null,"千兆","千兆","千兆","千兆","千兆","千兆"]
[null,null,"接口",null,"PCI-E","PCI-E","PCI-E","PCI-E","PCI-E","PCI-E"]
["操作系统",null,"正版操作系统",null,"正版操作系统","正版操作系统","正版操作系统","正版操作系统","正版操作系统","正版操作系统"]
["颜色",null,"显示器和机箱颜色",null,"黑色或灰色","黑色或灰色","黑色或灰色","黑色或灰色","黑色或灰色","黑色或灰色"]
["噪音",{"$nulls":3},"平均＜35dB","平均＜35dB","平均＜35dB","平均＜35dB","平均＜35dB","平均＜35dB"]
["辐射",{"$nulls":3},"GB9254-2008","GB9254-2008","GB9254-2008","GB9254-2008","GB9254-2008","GB9254-2008"]
["机箱尺寸",{"$nulls":3},"可立可卧中型机箱","可立可卧中型机箱","可立可卧中型机箱","AIO","AIO","塔式机箱≤25L"]
["USB",null,null,"规格/数据","≥6个","≥6个","≥6个","≥6个","≥6个","≥6个"]
["软驱",{"$nulls":3},"有","有","有","有","有","有"]
["电源",null,null,"类型","≤320W","≤320W","≤320W","≤320W","≤320W","≤320W"]
["鼠标",null,null,"接口类型","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)"]
[{"$nulls":3},"工作方式","光电","光电","光电","光电","光电","光电"]
["键盘",null,null,"接口类别","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)","有线（USB)"]
["声卡",{"$nulls":3},"内置集成声卡","内置集成声卡","内置集成声卡","内置集成声卡","内置集成声卡","内置集成声卡"]
[]
["PCI-E",{"$nulls":3},"有","有","有","有","有","有"]
["PCI槽",{"$nulls":3},"有","有","有","有","有","有"]
["一键恢复",{"$nulls":3},"有","有","有","有","有","有"]
["服务支持",{"$nulls":3},"售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:≥3年5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；故障报修后两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]
["特殊要求",{"$nulls":8},"公安部销售许可证、密码管理局认证、保密局认证证书\n"]
[]
["二、部门通用配置指标"]
["　　　部门通用配置标准不超过预算购置费限额，台式计算机部门通用配置标准不能超过6000元，主要用于满足部门日常办公使用过程中对计算机功能上的需求，在标准配置的基础上仅对有无光驱、USB接口数量等功能指标进行选择。"]
[null,null,"配置",null,"通用特殊配置可选"]
["显示器",null,"尺寸",null,"可选无显示器、19英寸宽屏、19英寸普屏、20英寸宽屏、21.5英寸、22英寸"]
[]
["光驱",null,"类型",null,"可选无光驱、DVD只读或者刻录"]
["网卡",null,"无线网卡",null,"可选"]
["操作系统",{"$nulls":3},"Windows 8"]
[{"$nulls":4},"windows 7"]
[{"$nulls":4},"winXP home"]
[{"$nulls":4},"winxp pro"]
[{"$nulls":4},"DOS"]
[{"$nulls":4},"Linux"]
["颜色",null,"显示器和机箱颜色固定为黑色或灰色",null,"黑色或灰色"]
["并口",{"$nulls":3},"可选"]
["PS/2接口",{"$nulls":3},"可选"]
["机箱尺寸",{"$nulls":3},"可选可立可卧中型机箱或塔式(立式)机箱。"]
["USB",null,null,"规格/数据","可选择个数"]
["显示器内置音箱",{"$nulls":3},"可选"]
["显示器是否能悬挂",{"$nulls":3},"可支持悬挂"]
["显示器是否能旋转 ",{"$nulls":3},"可支持旋转"]
["鼠标",null,null,"接口类型","无线"]
[{"$nulls":4},"有线USB"]
[{"$nulls":4},"有线PS/2"]
[{"$nulls":3},"工作方式","激光"]
[]
["键盘",null,null,"接口类别","无线或有线PS/2或者有线USB"]
["读卡器",{"$nulls":3},"可选"]
["摄像头",null,null,"　否","可选"]
["PCI-E",{"$nulls":3},"有"]
["PCI槽",{"$nulls":3},"有"]
["BIOS远程管理",{"$nulls":3},"可选"]
["一键恢复",{"$nulls":3},"有"]
[]
["三、部门专用配置指标"]
["台式计算机的部门专用配置标准主要用于满足测绘、科研等特殊用途需求，需要有财政部批复的专门预算，可以超过预算购置费限额（即6000元/台），在标准配置的基础上针对影响性能的指标进行调整，如CPU速率、内存大小、硬盘大小等，也可选择部门通用配置指标。"]
[null,null,"配置",null,"专用配置可选\n"]
["显示器",null,"尺寸",null,"19英寸"]
[{"$nulls":4},"20英寸"]
[{"$nulls":4},"21.5英寸"]
[{"$nulls":4},"22英寸"]
["硬盘",null,"硬盘容量",null,"1TB"]
[{"$nulls":4},"2TB"]
[{"$nulls":4},"4TB"]
["内存",null,"容量",null,"4GB"]
[{"$nulls":4},"8GB"]
["显卡",null,"类型",null,"独立显卡"]
["特殊要求",{"$nulls":3},"双网隔离机型"]
["CPU",{"$nulls":3},"可选择2.6GHZ、3.0GHZ、3.2GHZ，双核或四核CPU"]
["操作系统",{"$nulls":3},"Windows 8"]
[{"$nulls":4},"windows 7"]
[{"$nulls":4},"winXP home"]
[{"$nulls":4},"winxp pro"]
[{"$nulls":4},"DOS"]
[{"$nulls":4},"Linux"]

{"sheet":"便携式","index":1,"n_rows":80,"n_cols":10,"rows_kept":80,"merged":[[0,0,0,11],[1,0,1,13],[2,0,3,1],[2,2,3,3],[2,7,2,8],[2,9,2,11],[3,6,3,8],[3,9,3,11],[4,0,10,1],[4,2,4,3],[4,7,4,8],[4,9,4,11],[5,2,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,7,6,8],[5,9,6,11],[7,2,8,3],[7,4,8,4],[7,5,8,5],[7,6,8,6],[7,7,8,8],[7,9,8,11],[9,2,10,3],[9,4,10,4],[9,5,10,5],[9,6,10,6],[9,7,10,8],[9,9,10,11],[11,0,16,1],[11,2,12,3],[11,4,12,4],[11,5,12,5],[11,6,12,6],[11,7,12,8],[11,9,12,11],[13,2,13,3],[13,7,13,8],[13,9,13,11],[14,2,14,3],[14,7,14,8],[14,9,14,11],[15,2,16,3],[15,4,16,4],[15,5,16,5],[15,6,16,6],[15,7,16,8],[15,9,16,11],[17,0,22,1],[17,2,17,3],[17,7,17,8],[17,9,17,11],[18,2,18,3],[18,7,18,8],[18,9,18,11],[19,2,20,3],[19,4,20,4],[19,5,20,5],[19,6,20,6],[19,7,20,8],[19,9,20,11],[21,2,22,3],[21,4,22,4],[21,5,22,5],[21,6,22,6],[21,7,22,8],[21,9,22,11],[23,0,26,1],[23,2,23,3],[23,7,23,8],[23,9,23,11],[24,2,24,3],[24,7,24,8],[24,9,24,11],[25,2,26,3],[25,4,26,4],[25,5,26,5],[25,6,26,6],[25,7,26,8],[25,9,26,11],[27,0,29,1],[27,2,28,3],[27,4,28,4],[27,5,28,5],[27,6,28,6],[27,7,28,8],[27,9,28,11],[29,2,29,3],[29,7,29,8],[29,9,29,11],[30,0,32,1],[30,2,31,3],[30,4,31,4],[30,5,31,5],[30,6,31,6],[30,7,31,8],[30,9,31,11],[32,2,32,3],[32,7,32,8],[32,9,32,11],[33,0,35,1],[33,2,34,3],[33,4,34,4],[33,5,34,5],[33,6,34,6],[33,7,34,8],[33,9,34,11],[35,2,35,3],[35,7,35,8],[35,9,35,11],[36,0,36,1],[36,2,36,3],[36,7,36,8],[36,9,36,11],[37,0,37,1],[37,2,37,3],[37,7,37,8],[37,9,37,11],[38,0,38,1],[38,2,38,3],[38,7,38,8],[38,9,38,11],[39,0,39,3],[39,7,39,8],[39,9,39,11],[40,0,40,3],[40,7,40,8],[40,9,40,11],[41,0,41,3],[41,7,41,8],[41,9,41,11],[42,0,42,3],[42,4,42,12],[43,0,43,3],[43,7,43,8],[43,9,43,11],[44,0,44,9],[44,10,44,12],[45,0,45,9],[46,0,46,3],[47,0,47,3],[48,0,50,2],[48,3,50,3],[48,5,50,5],[48,6,50,6],[48,7,50,7],[48,8,50,9],[48,10,50,12],[51,0,52,2],[51,3,52,3],[51,5,52,5],[51,6,52,6],[51,7,52,7],[51,8,52,9],[51,10,52,12],[53,0,54,2],[53,3,54,3],[53,5,54,5],[53,6,54,6],[53,7,54,7],[53,8,54,9],[53,10,54,12],[55,0,56,2],[55,3,56,3],[55,5,56,5],[55,6,56,6],[55,7,56,7],[55,8,56,9],[55,10,56,12],[57,0,60,2],[57,3,60,3],[57,5,60,5],[57,6,60,6],[57,7,60,7],[57,8,60,9],[57,10,60,12],[61,0,62,2],[61,3,62,3],[61,5,62,5],[61,6,62,6],[61,7,62,7],[61,8,62,9],[61,10,62,12],[63,0,64,2],[63,3,64,3],[63,5,64,5],[63,6,64,6],[63,7,64,7],[63,8,64,9],[63,10,64,12],[65,0,66,2],[65,3,66,3],[65,5,66,5],[65,6,66,6],[65,7,66,7],[65,8,66,9],[65,10,66,12],[67,0,68,2],[67,3,68,3],[67,5,68,5],[67,6,68,6],[67,7,68,7],[67,8,68,9],[67,10,68,12],[69,0,69,2],[70,0,70,2],[72,0,72,13],[73,0,73,6],[74,0,74,2],[75,0,75,2],[76,0,76,2],[77,0,77,2],[78,0,78,2],[79,0,79,2]],"flags":["formulas_cached_only"]}
["2013年便携式计算机配置参考"]
["一、基本配置"]
[null,null,"配置",null,"配置一","配置二","配置三","配置四",null,"配置五"]
[{"$nulls":4},"<4000","4000元-6000元","6000元-8000元",null,null,"8000元-10000元"]
[null,null,"尺寸",null,"14寸","14寸","14寸","12寸",null,"14寸"]
[null,null,"分辨率",null,"≥1366*768","≥1366*768","≥1366*768","≥1366*768",null,"≥1600*900"]
[]
[null,null,"是否能旋转 ",null,"否","否","否","否",null,"否"]
[]
[null,null,"触摸屏",null,"否","否","否","否",null,"否"]
[]
["CPU(intel AMD 对应)",null,"核心数",null,"≥双核","≥I3 双核或同档次AMD CPU","≥I5 双核或同档次AMD CPU","≥I5 双核或同档次AMD CPU",null,"≥I7 双核或同档次AMD CPU"]
[]
[null,null,"主频",null,"≥1.6GHz","≥2.0GHz","≥2.2GHz","≥2.2GHz",null,"≥2.4GHz"]
[null,null,"缓存类型",null,"三级缓存","三级缓存","三级缓存","三级缓存",null,"三级缓存"]
[null,null,"缓存容量",null,"≥2M","≥3M","≥3M","≥3M",null,"≥4M"]
[]
["硬盘",null,"容量",null,"≥320G ","≥320G ","≥500G","≥500G",null,"≥750G"]
[null,null,"接口类型",null,"SATA","SATA","SATA","SATA",null,"SATA"]
[null,null,"缓存",null,"≥8M","≥8M","≥8M","≥8M",null,"≥8M"]
[]
[null,null,"转速",null,"≥5400转","≥5400转","≥5400转","≥5400转",null,"≥5400转"]
[]
["内存",null,"容量",null,"≥4G","≥4G","≥4G","≥4G",null,"≥4G"]
[null,null,"频率",null,"≥DDRIII","≥DDRIII","≥DDRIII","≥DDRIII",null,"≥DDRIII"]
[null,null,"内存插槽数量",null,"≥2","≥2","≥2","≥2",null,"≥2"]
[]
["显卡",null,"类型",null,"集成显卡","集成显卡","独立显卡 ","集成显卡",null,"独立显卡  "]
[]
[null,null,"显存容量",{"$nulls":3},"≥1G",null,null,"≥1G"]
["光驱",null,"类型",null,null,"DVDRW","DVDRW","DVDRW",null,"DVDRW"]
[]
[null,null,"接口",null,"SATA","SATA","SATA","SATA",null,"SATA"]
["网卡",null,"无线网卡",null,"10/100/1000M自适应","10/100/1000M自适应","10/100/1000M自适应","10/100/1000M自适应",null,"10/100/1000M自适应"]
[]
[null,null,"有线网卡",null,"10/100/1000M自适应","10/100/1000M自适应","10/100/1000M自适应","10/100/1000M自适应",null,"10/100/1000M自适应"]
["操作系统",null,"　操作系统",null,"　正版操作系统","　正版操作系统","　正版操作系统","　正版操作系统",null,"　正版操作系统"]
["电池",null,"电池",null,"≥4芯","≥6芯","≥6芯","≥6芯",null,"≥6芯"]
["颜色",null,"商务主流色",null,"黑色或灰色","黑色或灰色","黑色或灰色","黑色或灰色",null,"黑色或灰色"]
["电脑包",{"$nulls":3},"黑色","黑色","黑色","黑色",null,"黑色"]
["鼠标",{"$nulls":3},"有线USB接口","有线USB接口","有线USB接口","有线USB接口",null,"有线USB接口"]
["颜色",{"$nulls":3},"商务主流色（黑色、灰色、银色）","商务主流色（黑色、灰色、银色）","商务主流色（黑色、灰色、银色）","商务主流色（黑色、灰色、银色）",null,"商务主流色（黑色、灰色、银色）"]
["服务支持",{"$nulls":3}," 售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:≥3年5*8小时技术支持服务；2小时电话响应，故障报修后第二个工作日现场服务；两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]
["重量",{"$nulls":3},"<2.4KG","<2.4KG","<2.4KG","<2.4KG",null,"<2.4KG"]
["二、部门通用配置指标"]
["    部门通用配置标准不超过预算购置费限额，便携式计算机部门通用配置标准不能超过10000元，主要用于满足部门日常办公使用过程中对计算机功能上的需求，在标准配置的基础上仅对有无光驱、USB接口数量等功能指标进行选择。"]
["尺寸",{"$nulls":3},"可以选择14寸或12寸"]
["光驱数量",{"$nulls":3},"可选内置、外置或无光驱"]
["USB",null,null,"规格/数据（特殊配置可选）",2]
[{"$nulls":4},3]
[{"$nulls":4},4]
["笔记本电脑材质",null,null,"　","全金属"]
[{"$nulls":4},"合成材料（ABS、碳纤维等）"]
["鼠标",null,null,"接口类型","无线"]
[{"$nulls":4},"有线（USB)"]
["多媒体读卡器",null,null,"　","有"]
[{"$nulls":4},"无"]
["视频接口",{"$nulls":3},"HDMI"]
[{"$nulls":4},"DP"]
[{"$nulls":4},"DVI"]
[{"$nulls":4},"VGA"]
["音频接口",{"$nulls":3},"有"]
[{"$nulls":4},"无"]
["摄像头",null,null,"　","有"]
[{"$nulls":4},"无"]
["mini PCI-E",{"$nulls":3},"有"]
[{"$nulls":4},"无"]
["一键恢复",{"$nulls":3},"有"]
[{"$nulls":4},"无"]
["电池",{"$nulls":3},"4芯 6芯 8芯"]
["操作系统",{"$nulls":3},"winxphome; winxp pro; win7; win8; DOS　linux"]
[]
["三、部门专用配置指标"]
["  便携式计算机的部门专用配置标准主要用于满足测绘、科研等特殊用途需求，需要有财政部批复的专门预算，可以超过预算购置费限额（即10000元/台），在标准配置的基础上针对影响性能的指标进行调整，如CPU速率、内存大小、硬盘大小等，也可选择部门通用配置指标。"]
[{"$nulls":3},"配置","专用配置可选\n"]
["CPU",{"$nulls":3},"I3 I5 I7 或同档次AMD CPU"]
["硬盘",{"$nulls":3},"320G 500G 1T"]
["内存",{"$nulls":3},"2G 4G "]
["尺寸",{"$nulls":3},"可以选择12寸或14寸"]
["操作系统",{"$nulls":3},"winxphome; winxp pro; win7; win8; DOS　linux"]

{"sheet":"打印机","index":2,"n_rows":32,"n_cols":8,"rows_kept":32,"merged":[[0,0,0,7],[1,0,1,9],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,13,1],[14,0,14,1],[15,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,21,1],[20,2,21,2],[20,3,21,3],[20,4,21,4],[20,5,21,5],[20,6,21,6],[20,7,21,7],[22,0,22,1],[23,0,23,1],[24,0,25,1],[24,2,25,2],[24,3,25,3],[24,4,25,4],[24,5,25,5],[24,6,25,6],[24,7,25,7],[26,0,28,1],[26,2,28,2],[26,3,28,3],[26,4,28,4],[26,5,28,5],[26,6,28,6],[26,7,28,7],[29,0,29,1],[29,2,29,7],[30,0,30,9],[31,1,31,2],[34,0,34,9]],"flags":["formulas_cached_only"]}
["2013年打印机配置参考"]
["一、基本配置"]
["技术指标",null,"A4激光黑白双面","A4激光黑白双面","A4激光彩色双面","A4彩色喷墨","A3激光黑白双面","A3激光彩色双面"]
["价格",null,"1000元","2500元","3500元","2500元","8000元","10000元"]
["首页输出时间",null,"≤8.5秒","≤8秒","黑白：≤18.5秒\n彩色：≤19秒",null,"<10秒","黑白≤16秒\n彩色≤17秒"]
["月打印负荷",null,"5000页","50000页","30000页","20000页","60000页","60000页"]
["打印速度（A4）",null,"14ppm","33ppm","彩色：14ppm\n黑白：14ppm ","黑白：26ppm\n彩色：24ppm","26ppm","彩色：20ppm\n黑白：20ppm "]
["物理分辨率",null,"600x600dpi","1200x1200dpi","600x600dpi","4800x1200dpi","600x600dpi","600x600dpi "]
["标配内存（内存必须内置，不可另配）",null,"2M","64M","128MB","64MB","64MB","448MB"]
["接口（接口必须内置，不可外接转换接口）",null,"USB 2.0 (接口内置)","USB 2.0 /100Base-TX（RJ-45网络接口）","USB 2.0 /100Base-TX（RJ-45网络接口）","USB 2.0 /100Base-TX（RJ-45网络接口）","USB 2.0 /100Base-TX（RJ-45网络接口）","USB 2.0 /100Base-TX（RJ-45网络接口）"]
["兼容系统",null,"Windows 2000/XP Home/XP Professional/XP Professional x64/Vista\nMac OS X 10.3.x/10.4或更高版本","Windows 2000/XP Home/XP Professional/Server 2003/Vista\nMac OS X v10.3.9/10.4/10.5\nunix\nlinux","Windows 7/Vista/XP /Server 2008/Server 2003\nMac OS X v10.5.8/v10.6/v10.7\nlinux","Windows XP/Vista/2008/2003/7\nMac OS X 10.4.11/10.5.x/10.6.x","Windows 98/Me/2000/XP/Vista/7/8","Windows 2000/XP Home/XP Professional/XP Media Center/XP Professional x64/Server 2003/Vista/7\nMac OS X v10.3-10.4或更高版本\nLinux "]
["硒鼓寿命",null,"1500页","2300页","黑色：1600页，\n蓝色/黄色/品红色：1800页","黑2400页\n彩1200页","10000页","黑色7000页\n彩色7300页"]
["电源功率",null,"无","无","无","无","无","无"]
[]
["网络打印",null,"否","是","是","是","是","是"]
["液晶显示屏"]
[]
["标配自动纸盒",null,1,2,1,1,1,2]
["标配进纸盒容量",null,"150页","250页",150,"250页","250页","250页"]
["标配出纸容量",null,"100页","150页","100页",null,"150页","100页"]
["自动双面打印",null,"是","是","是","是","是","是"]
[]
["支持介质尺寸",null,"A4，B5，A5，A6，明信片，信封（B5，C5，DL）","A4，B5，A5，A6，信封（B5，C5，DL）","A4，A5，A6，B5 (JIS)，16K；10x15厘米，明信片（JIS单面，JIS双面），信封 (DL，C5，B5) ","A4，A5，B5，Letter，Legal","A3，A4，A5，B4，B5，Letter，Legal，Executive，ledger，statement，长纸（297x900mm）","A3，B4，A4，B5，A5，A6，RA3，SRA3，10×15cm，信封（B5，C5，DL）"]
["支持介质类型",null,"普通纸，激光打印纸，牛皮纸，相纸，糙纸，投影胶片，信封，明信片，标签，卡片","普通纸，证券纸，轻质纸，重磅纸，再生纸，糙纸，重磅介质，投影胶片，信封，标签，卡片","证券纸，宣传册纸，彩纸，光面纸，重磅纸，信头纸，轻质纸，相纸，普通纸，预打印纸，预穿孔纸，再生纸，糙纸，投影胶片，标签，信封，卡片","普通纸，厚纸，信封，超级光泽照片纸，高质量光泽照片纸，高质量亚光照片纸，光泽照片纸，照片纸，不干胶贴纸","普通纸，厚纸，透明胶片，信封，卡片纸，再生纸，纸标签","普通纸，宣传册纸，证券纸，光面纸，预打印纸，预穿孔纸，再生纸，相纸，彩纸，糙纸，光面胶片，投影胶片，信封，信头纸，标签，卡片"]
["是否支持通用耗材",null,"是","是","是","是","是","是"]
[]
["机身颜色",null,"商务主流色，黑、灰、银、白等","商务主流色，黑、灰、银、白等","商务主流色，黑、灰、银、白等","商务主流色，黑、灰、银、白等","商务主流色，黑、灰、银、白等","商务主流色，黑、灰、银、白等"]
[]
[]
["服务支持",null,"售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:≥1年5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；故障报修后两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]
["二、部门通用配置指标"]
["接口","可选择并口"]

{"sheet":"空调机","index":3,"n_rows":26,"n_cols":13,"rows_kept":26,"merged":[[0,0,0,12],[1,0,1,12],[2,0,2,1],[3,0,3,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[19,2,19,12],[20,0,20,12],[21,0,21,5],[22,0,22,1],[22,2,22,5],[23,0,23,1],[23,2,23,5],[24,0,24,1],[24,2,24,5],[25,0,25,1],[25,2,25,5],[26,0,26,2]],"flags":["formulas_cached_only"]}
["2013年空调机配置参考"]
["一、基本配置"]
["配置",null,"分体定速壁挂机1","分体定速壁挂机2","分体定速壁挂机3","分体变频壁挂机1","分体变频壁挂机2","分体变频壁挂机3","分体定速柜机1","分体定速柜机2","分体定速柜机3","分体变频柜机1","分体变频柜机2"]
["价格",null,"2300元","3000元","5000元","3500元","4000元","7000元","5000元","7000元","10000元","7000元","9000元"]
["规格（匹数）",null,"1P","1.5P","2P","1P","1.5P","2P","2P","3P","5P","2P","3P"]
["额定制冷量（W）",null,"2500≤额定制冷量＜3200","3500≤额定制冷量＜5000","5000≤额定制冷量＜7200","2500≤额定制冷量＜3200","3500≤额定制冷量＜5000","5000≤额定制冷量＜7200","5000≤额定制冷量＜7200","7200≤额定制冷量＜12000","额定制冷量≥12000","5000≤额定制冷量＜7200","7200≤额定制冷量＜12000"]
["制冷面积",null,"10-15m2","16-24m2","22-34m2","10-15m2","16-24m2","22-34m2","22-34m2","32-50m2","46-70m2","22-34m2","32-50m2"]
["冷暖类型",null,"冷暖","冷暖","冷暖","冷暖","冷暖","冷暖","冷暖","冷暖","冷暖","冷暖","冷暖"]
["能效等级",null,"≥二级","≥二级","≥二级","≥二级","≥二级","≥二级","≥二级","≥二级","≥二级","≥二级","≥二级"]
["电辅加热",null,"支持","支持","支持","支持","支持","支持","支持","支持","支持","支持","支持"]
["颜色",null,"白色","白色","白色","白色","白色","白色","白色","白色","白色","白色","白色"]
["随机配插头/空开",null,"220V插头","220V插头","220V空气开关","220V插头","220V插头","220V空气开关","220V空气开关","220V空气开关","380V空气开关","220V空气开关","220V空气开关"]
["随机连接管长度",null,"≥2.5米","≥2.5米","≥2.5米","≥2.5米","≥2.5米","≥2.5米","≥4.5米","≥4.5米","≥4.5米","≥4.5米","≥4.5米"]
["随机水管长度",null," ≥ 3米"," ≥ 4米"," ≥ 5米"," ≥ 6米"," ≥ 7米"," ≥ 8米"," ≥ 5米"," ≥ 5米"," ≥ 5米"," ≥ 5米"," ≥ 5米"]
["随机电源线长度",null,"1.5米","1.5米","1.5米","1.5米","1.5米","1.5米","1.5米","1.5米","1.5米","1.5米","1.5米"]
["连接管加长价格（包括高低压管路、保温套、连接线、焊接、缠带、加长管部加冷媒等）",null,"75元/米","75元/米","100元/米","75元/米","75元/米","100元/米","100元/米","120元/米","150元/米","100元/米","120元/米"]
["水管加长价格",null,"10元/米","10元/米","10元/米","10元/米","10元/米","10元/米","10元/米","10元/米","10元/米","10元/米","10元/米"]
["电源线加长价格",null,"10元/米","10元/米","15元/米","10元/米","10元/米","15元/米","15元/米","25元/米","30元/米","15元/米","25元/米"]
["支架（含地角、膨胀螺丝）",null,"25元","25元","25元","25元","25元","25元","25元","35元","60元","25元","35元"]
["售后服务",null,"售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:整机六年质保；5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；故障报修后两个工作日解决问题。免费送货到中央单位指定的地点，免费上门勘查设计安装方案，免费安装。安装过程中免费打孔（砖墙），混凝土和玻璃打孔不超过50元/个，拆装护栏/门不超过100元，拆除原有旧机不超过100元/台，免收高空作业费。因加长连接管需要加注冷媒的不再另行收费。"]
["二、部门通用配置指标"]
["　　　部门通用配置标准不超过预算购置费限额，主要用于满足部门日常办公使用过程中对空调功能上的需求，在标准配置的基础上仅对有无独立抽湿等功能指标进行选择。"]
["配置",null,"部门通用配置指标"]
["独立除湿",null,"可选"]
["冷暖类型",null,"可选单冷"]
["电源",null,"220V、380V"]

{"sheet":"复印机","index":4,"n_rows":31,"n_cols":8,"rows_kept":31,"merged":[[0,0,0,7],[1,0,1,16],[18,0,19,0],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,4],[18,5,19,5],[18,6,19,6],[18,7,19,7],[20,0,21,0],[23,0,24,0],[23,1,24,1],[23,2,24,2],[23,3,24,3],[23,4,24,4],[23,5,24,5],[23,6,24,6],[23,7,24,7],[25,0,26,0],[29,1,29,7],[30,1,30,7],[33,0,33,6],[35,0,35,6]],"flags":["formulas_cached_only"]}
["2013年复印机配置参考"]
["一、基本配置"]
["配置参数","配置一","配置二","配置三","配置四","配置五","配置六","配置七"]
[null,"A4黑白复印机","A3黑白复印机Ⅰ","A3黑白复印机Ⅱ","A3黑白复印机Ⅲ","A3黑白复印机Ⅳ","A3彩色复印机Ⅰ","A3彩色复印机Ⅱ"]
["价格","10000元","10000元","15000元","25000元","35000元","25000元","35000元"]
["是否带硬盘","不带","不带","不带","不带","不带"]
["复印速度","≥30页/分钟","≥18页/分钟","≥25页/分钟","≥ 35页/分钟","≥45页/分钟","≥20页/分钟","≥30页/分钟"]
["双面自动送稿器","≥50页","≥51页","≥50页","≥50页","≥100页","≥50页","≥50页"]
["待机首页复印时间","≤9 秒","≤9 秒","≤ 8秒","≤ 5秒","≤ 5秒","黑白≤ 10秒；彩色≤ 11秒","黑白≤ 10秒；彩色≤ 11秒"]
["复印分辨率","≥600*600dpi","≥600*600dpi","≥600*600dpi","≥600*600dpi","≥600*600dpi","≥600*600dpi","≥600*600dpi"]
["ID卡复印功能","支持","支持","支持","支持","支持","支持","支持"]
["内存容量","≥256 MB","≥256 MB","≥128MB","≥512MB","≥512MB","≥512MB","≥1G"]
["双面器",null,null,"标配","标配","标配","标配","标配"]
["纸张容量","≥300页","≥300页","≥600页","≥1100页","≥1000页","≥600页","≥600页"]
["缩放比率","25-400%","50-200%","25-400%","25% - 400%","25% - 400%","25-400%","25-400%"]
["接口（接口内置）","USB","USB","USB","USB+网络","USB+网络","USB+网络","USB+网络"]
["预热时间","≤ 25秒","≤ 25秒","≤ 25秒","≤ 25秒","≤ 25秒","≤ 25秒","≤ 25秒"]
["耗材描述","支持通用耗材","支持通用耗材","支持通用耗材","支持通用耗材","支持通用耗材","支持通用耗材","支持通用耗材"]
["扫描功能","支持黑白和彩色扫描","支持黑白和彩色扫描","支持黑白和彩色扫描","支持黑白和彩色扫描","支持黑白和彩色扫描","支持黑白和彩色扫描","支持黑白和彩色扫描"]
[]
["扫描方式","本地扫描","本地扫描","本地扫描","本地扫描","本地扫描","本地扫描","本地扫描"]
[{"$nulls":5},"网络扫描"]
["面板颜色","黑白","黑白","黑白","黑白","黑白","黑白","黑白"]
["打印功能",null,null,"本地","本地、有线网络","本地、有线网络","本地","本地"]
[]
["装订器","平钉、角钉","平钉、角钉","平钉、角钉","平钉、角钉","平钉、角钉","平钉、角钉","平钉、角钉"]
[null,"骑马钉（小册子装订功能）","骑马钉（小册子装订功能）","骑马钉（小册子装订功能）","骑马钉（小册子装订功能）","骑马钉（小册子装订功能）","骑马钉（小册子装订功能）","骑马钉（小册子装订功能）"]
["打孔","是","是","是","是","是","是","是"]
["颜色","灰白","灰白","灰白","灰白","灰白","灰白","灰白"]
["特殊要求","预算单位选择和使用相关配置机型必须符合国务院相关保密规定。"]
["售后服务","售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:5*8小时技术支持服务；2小时电话响应，故障报修后第二个工作日现场服务；两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]

{"sheet":"传真机","index":5,"n_rows":22,"n_cols":3,"rows_kept":22,"merged":[[0,0,0,2],[1,0,1,13],[4,0,9,0],[7,1,8,1],[7,2,8,2],[10,0,14,0],[10,1,11,1],[10,2,11,2],[15,0,17,0],[18,0,19,0],[18,1,19,1],[18,2,19,2],[21,1,21,2],[22,0,22,6],[23,0,23,6]],"flags":["formulas_cached_only"]}
["2013年传真机配置参考"]
["一、基本配置"]
[null,"配置参数","配置一"]
[null,"价格","2000元"]
["基本参数","自动输稿器","≥20页(A4)"]
[null,"供纸容量","≥150张(A4)"]
[null,"内存","≥16MB"]
[null,"机身颜色","商务主流色，黑色、灰色、银色、白色。"]
[]
[null,"语言","中文"]
["传真功能参数","传输速度\n（调制解调器）","≥33.6Kbps"]
[]
[null,"传真分辨率","≥300*300dpi"]
[null,"快速拨号","支持"]
[null,"文稿尺寸"]
["打印功能参数","是否支持打印","支持"]
[null,"打印速度（A4)","≥14页/分钟"]
[null,"打印分辨率","≥600dpi*600dpi"]
["复印功能参数","是否支持复印","支持"]
[]
[]
["服务支持","售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:5*8小时技术支持服务；2小时电话响应，故障报修后第二个工作日现场服务；两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]

{"sheet":"扫描仪","index":6,"n_rows":39,"n_cols":6,"rows_kept":39,"merged":[[0,0,0,5],[1,0,1,13],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,5],[9,0,10,0],[11,0,13,0],[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,5,15,5],[16,0,21,0],[16,1,21,1],[16,2,21,2],[16,3,21,3],[16,4,21,4],[16,5,21,5],[23,0,24,0],[23,1,24,1],[23,2,24,2],[23,3,24,3],[23,4,24,4],[23,5,24,5],[25,0,26,0],[25,1,26,1],[25,2,26,2],[25,3,26,3],[25,4,26,4],[25,5,26,5],[27,0,28,0],[27,1,28,1],[27,2,28,2],[27,3,28,3],[27,4,28,4],[27,5,28,5],[33,0,34,0],[33,1,34,1],[33,2,34,2],[33,3,34,3],[33,4,34,4],[33,5,34,5],[35,0,37,0],[35,1,37,1],[35,2,37,2],[35,3,37,3],[35,4,37,4],[35,5,37,5],[38,1,38,5],[42,0,42,6],[46,0,46,6]],"flags":["formulas_cached_only"]}
["2013年扫描仪配置参考"]
["一、基本配置"]
["配置参数","平板扫描仪Ⅰ","平板扫描仪Ⅱ","高速扫描仪Ⅰ","高速扫描仪Ⅱ","高速扫描仪Ⅲ"]
["价格","800元","2000元","3000元","3000元","4000元"]
["扫描方式","平板","平板","ADF+平板","ADF","ADF"]
[]
[null,"A4","A4","A4","A4","A4"]
["扫描元器件","CCD或者CIS","CCD或者CIS","CCD或者CIS","CCD或者CIS","CCD或者CIS"]
[]
["扫描光源"]
[]
["色彩位数"]
[]
[]
["最大光学分辨率","≥1200dpi ","≥1200dpi ","≥1200dpi ","≥1200dpi ","≥1200dpi "]
[]
["高度文档扫描速度（200dpi，黑白，灰度，彩色同速）",null,null,"≥ 15ppm/30ipm","≥ 20ppm/40ipm","≥ 30ppm/60ipm"]
[]
[]
[]
[]
[]
["扫描介质","文件,图片,证件","文件,图片,证件","文件,图片,证件","文件,图片,证件","文件,图片,证件"]
["双面扫描",null,null,"双面","双面","双面"]
[]
["网络扫描"]
[]
["日处理量",null,null,"≥1000页","≥1000页","≥2000页"]
[]
["文件输出格式","支持JPG、TIFF、多页PDF","支持JPG、TIFF、多页PDF","支持JPG、TIFF、BMP、多页PDF","支持JPG、TIFF、BMP、多页PDF","支持JPG、TIFF、BMP、多页PDF"]
["动态存储格式"]
["接口方式","USB2.0接口","USB2.0接口","USB2.0接口","USB2.0接口","USB2.0接口"]
["影像处理软件功能","自动纠偏、自动裁切、自动去噪","自动纠偏、自动裁切、自动去噪","自动纠偏、自动裁切、自动去噪","自动纠偏、自动裁切、自动去噪","自动纠偏、自动裁切、自动去噪"]
["随机软件（驱动软件、图像编辑软件、文字识别软件、\n电子手册等）","有","有","有","有","有"]
[]
["ADF容量",null,null,"≥50页","≥50页","≥50页"]
[]
[]
["服务支持","售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；故障报修后两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]

{"sheet":"复印纸","index":7,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[0,0,0,4],[1,0,1,13],[4,0,9,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,7,4],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,9,4],[10,0,16,0],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,0,18,0],[17,1,18,1],[17,2,18,4],[19,0,19,6],[21,0,27,0],[21,1,23,1],[21,2,23,2],[24,1,25,1],[24,2,25,2],[26,1,27,1],[26,2,27,2],[30,0,30,6]],"flags":["formulas_cached_only"]}
["2013年复印纸配置参考（京内单位执行）"]
["一、基本配置"]
[null,"配置参数","配置一","配置二","配置三"]
["价格（每箱）",null,"140元","220元","100元"]
["基本参数","纸张大小","A4","A3","B5"]
[]
[null,"纸张定量","70g","70g","70g"]
[]
[null,"纸张用浆","全木浆","全木浆","全木浆"]
[]
["其他参数","不透明度","符合GB/T 24988-2010《复印纸》合格品要求"]
[null,"挺度","符合GB/T 24988-2011《复印纸》合格品要求"]
[null,"定量及定量偏差","符合GB/T 24988-2012《复印纸》合格品要求"]
[null,"厚度","符合GB/T 24988-2013《复印纸》合格品要求"]
[null,"内容量偏差","符合GB/T 24988-2014《复印纸》合格品要求"]
[null,"尘埃度","符合GB/T 24988-2015《复印纸》合格品要求"]
[null,"规格","5包/箱，每包500张纸"]
["服务支持",null,"售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；免费送货到中央单位指定的地点。"]
[]
["二、部门通用配置指标"]
[null,"配置","部门通用配置指标"]
["基本参数","纸张大小","可选B4、8K、16K"]
[]
[]
[null,"纸张定量","可选80g"]
[]
[null,"纸张用浆","可选混浆、再生纸"]

{"sheet":"碎纸机","index":8,"n_rows":20,"n_cols":4,"rows_kept":20,"merged":[[0,0,0,4],[1,0,1,13],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,3,10,3],[11,0,12,0],[11,1,12,1],[11,2,12,2],[11,3,12,3],[14,0,18,0],[19,1,19,3],[21,0,21,6],[23,0,23,6]],"flags":["formulas_cached_only"]}
["2013年碎纸机配置参考(京内单位执行)"]
["一、基本配置"]
["配置参数","配置一","配置二","配置三"]
["价格","1200元","1600元","2000元"]
["碎纸方式","颗粒状或段状","颗粒状或段状","颗粒状或段状"]
[]
["入口宽度"," >=A4"," >=A4"," >=A4"]
["碎纸能力","一次>=8张纸（A4,70g）、1张光盘以上","一次>=10张纸（A4,70g）、1张光盘以上","一次>=15张纸（A4,70g）、3张光盘以上"]
["工作持久力","连续碎纸时间>=8分钟 ","连续碎纸时间>=15分钟","连续碎纸时间>=20分钟"]
["碎纸速度","2M/分钟","2M/分钟","3M/分钟"]
[]
["碎纸箱容积",">= 17L ",">= 20L",">= 20L"]
[]
["工作噪音","<=60DB","<=60DB","<=60DB"]
["其他特性","入纸过量，自动退纸","入纸过量，自动退纸","入纸过量，自动退纸"]
[null,"可碎大头针，曲别针","可碎大头针，曲别针","可碎大头针，曲别针"]
[null,"可碎书钉、信用卡","可碎书钉、信用卡","可碎书钉、信用卡"]
[null,"过热停机","过热停机","过热停机"]
[null,"门开断电保护","门开断电保护","门开断电保护"]
["服务支持","售后服务标准必须与该产品出厂市场标准服务一致,同时还应包括:5*8小时技术支持服务；2小时电话响应，第二个工作日现场服务；故障报修后两个工作日解决问题，否则在三个工作日内提供备机,免费送货到中央单位指定的地点。"]